{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["8"],"not_rendered":{"charts":1,"images":16,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"8","index":0,"n_rows":28,"n_cols":22,"rows_kept":28,"cut":false,"hidden":false,"merged":[[7,2,15,2]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,"This calculation is designed to help demonstrate the effects of pressure drop on the operating cost of air treatment products such as air dryers and filters.      It is also important to consider not only the initial, but also the saturated and recommended filter element change pressure drop when calculating the electrical cost"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Flow",null,null,"Pressure",null,null,"Currency"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,false,"l/s",1,false,"bar",1,false,"€"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,false,"m³/hr",0.27777800000000002,true,"psi",6.8965520000000002E-2,true,"$"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,false,"m³/min",16.666667,null,null,null,false,"£"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,true,"cfm",0.47169800000000001,null,null,null,false,"Other"]
[]
[null,null,"Units Of Measure"]
[null,null,"Pressure","Flow",null,null,null,null,null,null,null,null,null,null,{"$f":"IF($U$16=TRUE,$F$20,\"XXX\")","v":"XXX"}]
[null,null,"Currency",{"$f":"IF(U16=TRUE,\"Type currency here ======>\",\"\")","v":""},null,"xx"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Converted flow",{"$f":"IF(O13=TRUE,E23*Q13,IF(O14=TRUE,E23*Q14,IF(O15=TRUE,E23*Q15,E23*Q16)))","v":463.20743600000003},null,"Converted pressure 1",{"$f":"IF($R$13=TRUE,E24*$T$13,E24*$T$14)","v":8.4827589600000003E-2}]
[null,null,"Operating Conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Converted pressure 2",{"$f":"IF($R$13=TRUE,#REF!*$T$13,#REF!*$T$14)","v":{"$error":"#REF!"}}]
[null,null,"Flow through the dryer/filter",null,982,{"$f":"VLOOKUP(TRUE,O13:P16,2,FALSE)","v":"cfm"}]
[null,null,"Pressure drop dryer/filter",null,{"$f":"G24/100","v":1.23},{"$f":"VLOOKUP(TRUE,$R$13:$S$14,2,FALSE)","v":"psi"},123]
[null,null,"Price per kWh",null,{"$f":"G25/1000","v":1.6E-2},{"$f":"IF(VLOOKUP(TRUE,U13:V16,2,FALSE)=\"OTHER\",IF(F20=\"\",\"No Currency\",F20),(VLOOKUP(TRUE,U13:V16,2,FALSE)))","v":"$"},16]
[null,null,"Running hours per year",null,8000,"hours"]
[]
[null,null,"Pressure drop dryer/filter",null,{"$f":"(S21/0.1)*P21*E26*0.35*0.007*E25","v":123.22212760020076},{"$f":"IF(F25=\"No Currency\",\"\",CONCATENATE(F25,\"/year\"))","v":"$/year"}]